### <=========================================================================================> ### ###---> version [carlos @ mdc-homestation ~] $ Sun Mar 16 16:09:17 BRT 2014 = == == == == == == == == == == > ### ###---> PMTA Installer + Interspire revised March 16, 2014 by == == == == == == == == == == = > ### ###---> Mundocloud Cloud Solutions-information about this script: == == == == == == == == == == == > ### ###---> http://www.mundocloud.com.br or by email: contato@mundocloud.com.br = == == == == == == == > ### ### <=========================================================================================> ### ### <=========================================================================================> ### ###---> preparing the machine = == == == == == == == == == == == == == == == == == == == == == == == == == == == == == == == > ### ### < === === === === === === === === === === === === === === === === === === === === === == == == == == == == == == == == == == > ### 1---> Install CentOS 5X64 or 6X64 in single partition, that is, do not separate the '/home ', '/var ', '/root ' '//root ' are the maintenance scripts and backups, the/home are e-mail boxes and hosting, in/var are the spools, send the logs, DNS and others essential services, So it is essential to leave enough space for these directories on this measure : 70% to 15%/var 15%/root to the/home the HD must have at least 100 GB for sending daily emails with 1 mm 3 64IPS---> IP Configuration in the network-3-the = If the IPs are separated (few ips/no range):-Clone the file/etc/sysconfig/network-scripts/ifcfg-eth0 to/etc/sysconfig/network-scripts/ifcfg-eth0:0 or/etc/sysconfig/network-scripts/ifcfg-venet0 for/etc/sysconfig/network-scripts/ifcfg-venet0:0 by editing a file for each IP.

	-3-B = case use a range of IPs separated or varied, for example 188.165.92.0, 188.165.92.10, 188.165.92.22, 188.165.92.43:-3-B-1 = Clone the file/etc/sysconfig/network-scripts/ifcfg-eth0 to/etc/sysconfig/network-scripts/ifcfg-eth0:0 or/etc/sysconfig/network-scripts/ifcfg-venet0 for/etc/sysconfig/network-scripts/ifcfg-venet0:0 and configure each valid ip range, in a file as in the example would be "188.165.92.0" 1: DEVICE = eth0:0 (or venet0:0 = number of the interface)
	BOOTPROTO = static IPADDR = 188.165.92.0 (IP) NETMASK = 255.255.255.128 (Mask of the range) = 188.165.92.254 GATEWAY (the Gateway range) BROADCAST = 188.165.92.255 (Broadcast of range) ONBOOT = yes 2 example would be "188.165.92.10": DEVICE = eth0:0 (or venet0:1 = number of the interface)
	BOOTPROTO = static IPADDR = 188.165.92.10 (IP) NETMASK = 255.255.255.128 (Mask of the range) = 188.165.92.254 GATEWAY (the Gateway range) BROADCAST = 188.165.92.255 (Broadcast of range) ONBOOT = yes-3-B-2 = If you use a range of ips with number followed, you can create the file:/etc/sysconfig/network-scripts/ifcfg-eth0-range0 or/etc/sysconfig/network-scripts/ifcfg-venet0-range0, setting up the first valid ip range until the last following the instruction below : DEVICE = eth0-range0 (or venet0-range0 = interface name) BOOTPROTO = static IPADDR_START = 188.165.92.1 (first valid ip range) IPADDR_END = 188.165.92.128 (last valid ip range) NETMASK = 255.255.255.128 (Mask of the range) CLONENUM_START = 0 (eth0:0 or venet0:0 = first interface to be created) ONBOOT = yes # ## <=========================================================================================> ### ###---> System Setup ### <=========================================================================================> ###-Access the server/root;
	-Unzip the Installer package that is zipped, run unzip-q "zipado.zip package";
	-Give full permission chmod 777 recursive "arquivo.sh" for the uncompressed installation script;
	-Follow the instructions that appear on the screen.

5---> commands to Setup: unzip *.zip q-chmod 777 *.sh & & & &./*.sh ### <=========================================================================================> ###

